	cmdinv
	cmd
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struct stByte
 {
   unsigned char AddressL; //Lower Address
   unsigned char AddressH; 
   unsigned char cmd;
   unsigned char cmdinv; //Higher Address
 } ;
typedef  struct stByte  BYTES;
BYTES   iRcode;

Example:
iRcode.AddressL=0x01;
iRcode.AddressH=0xFE;
iRcode.cmd=0x10;
iRcode.cmdinv=0XEF;

	uL

	cmdinv
	cmd
	AddressH
	AddressL


union unLONGINT
 {
  unsigned long   uL; //4 bytes
  BYTES  b; //4 bytes
 };
typedef  union unLONGINT  LONGUNION ;
LONGUNION  iRcodeL;

iRcodeL.b=iRcode;

iRcodeL.uL  相當於0xEF10FE01
